{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet4","Sheet2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":35,"n_cols":7,"rows_kept":35,"cut":false,"hidden":false,"merged":[]}
["Module","Configuration Item","Type","Expect Value","Search Pattern","Search Text","Search Rule"]
["Dcm","DcmResetToFblAfterSessionFinalResponseEnabled","FIXED_VALUE","true","NA","NA","NA"]
["Dcm","DcmSpecificCauseCodeEnabled","FIXED_VALUE","true","NA","NA","NA"]
["Dem","DemResetConfirmedBitOnOverflow","FIXED_VALUE","false","NA","NA","NA"]
["Dem","DemPendingDtcProcessing","FIXED_VALUE","DEM_PROCESS_PDTC_ALL_DTC","NA","NA","NA"]
["Dem","DemWarningIndicatorRequestedProcessing","FIXED_VALUE","DEM_PROCESS_WIR_ALL_DTC","NA","NA","NA"]
["Dcm","DcmSpecificCauseCodeEnabled","FIXED_VALUE","true","NA","NA","NA"]
["Dem","DemClearDTCBehavior","FIXED_VALUE","DEM_CLRRESP_VOLATILE","NA","NA","NA"]
["Dem","DemMaxNumberEventEntryPrimary","FIXED_VALUE","40","NA","NA","NA"]
["Dem","DemTypeOfFreezeFrameRecordNumeration","FIXED_VALUE","DEM_FF_RECNUM_CONFIGURED","NA","NA","NA"]
["Dem","DemImmediateNvStorage","FIXED_VALUE","true","NA","NA","NA"]
["CanTp","CanTpChannelMode","FIXED_VALUE","CANTP_MODE_FULL_DUPLEX","NA","NA","NA"]
["CanTp","CanTpMainFunctionPeriod","FIXED_VALUE","0.005","NA","NA","NA"]
["CanTp","CanTpEnableSynchronousTransmit","FIXED_VALUE","true","NA","NA","NA"]
["EthIf","EthIfVlanId","FIXED_VALUE","7","NA","NA","NA"]
["EthIf","EthIfTrcvLinkStateChgMainReload","FIXED_VALUE","50","NA","NA","NA"]
["EthTrcv","EthTrcvHwAccessMonitorPeriod","FIXED_VALUE","1","NA","NA","NA"]
["DoIP","DoIPControlIpAssignment","FIXED_VALUE","false","NA","NA","NA"]
["DoIP","DoIPTcpTxMgtQueueSize","FIXED_VALUE","31","NA","NA","NA"]
["Rte","RteExclusiveAreaImplMechanism","CUSTOM_PATTERN","NONE",".//SHORT-NAME","ETHTRCV_30_88Q1010_EXCLUSIVE_AREA_SEQUENCE","CONTAINS"]
["Rte","RteExclusiveAreaImplMechanism","CUSTOM_PATTERN","NONE",".//SHORT-NAME","ETHTRCV_30_88Q1010_EXCLUSIVE_AREA_SEQUENCE","CONTAINS"]
["Rte","RteExclusiveAreaImplMechanism","CUSTOM_PATTERN","NONE",".//SHORT-NAME","EXCLUSIVE_AREA_SMI_MULTI_CHIP_ACCESS","CONTAINS"]
["TcpIp","TcpIpAssignmentTrigger","CUSTOM_PATTERN","TCPIP_MANUAL",".//SHORT-NAME","NE_CCP_MCU","CONTAINS"]
["ComM","ComMMainFunctionPeriod","FIXED_VALUE","0.01","NA","NA","NA"]
["ComM","ComMNmVariant","CUSTOM_PATTERN","FULL",".//SHORT-NAME","CNCANConnector","CONTAINS"]
["ComM","ComMNmVariant","CUSTOM_PATTERN","FULL",".//SHORT-NAME","ADCANFDConnector","CONTAINS"]
["ComM","ComMNmVariant","CUSTOM_PATTERN","FULL",".//SHORT-NAME","CHCANFDConnector","CONTAINS"]
["ComM","ComMNmVariant","CUSTOM_PATTERN","FULL",".//SHORT-NAME","CFCANConnector","CONTAINS"]
["ComM","ComMNmVariant","CUSTOM_PATTERN","LIGHT",".//SHORT-NAME","DIAGCANConnector","CONTAINS"]
["ComM","ComMNmVariant","CUSTOM_PATTERN","FULL",".//SHORT-NAME","PTEXTCAN","CONTAINS"]
["ComM","ComMNmVariant","CUSTOM_PATTERN","FULL",".//SHORT-NAME","PTCAN","CONTAINS"]
["ComM","ComMNmVariant","CUSTOM_PATTERN","LIGHT",".//SHORT-NAME","Lin2","CONTAINS"]
["ComM","ComMNmVariant","CUSTOM_PATTERN","LIGHT",".//SHORT-NAME","LIN1","CONTAINS"]
["Ea","EaNumberOfWriteCycles","FIXED_VALUE","1000000","NA","NA","NA"]
["CanIf","test_key","DEPENDENCY_PATTERN","test_value","Search Pattern","NA","Search Rule"]

{"sheet":"Sheet4","index":1,"n_rows":11,"n_cols":3,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
["('Dem'","DemMaxNumberEventEntryPrimary","40"]
["('Dem'","DemTypeOfFreezeFrameRecordNumeration","DEM_FF_RECNUM_CONFIGURED"]
["('Dem'","DemImmediateNvStorage","true"]
["('CanTp'","CanTpChannelMode","CANTP_MODE_FULL_DUPLEX"]
["('CanTp'","CanTpMainFunctionPeriod","0.005"]
["('CanTp'","CanTpEnableSynchronousTransmit","true"]
["('EthIf'","EthIfVlanId","7"]
["('EthIf'","EthIfTrcvLinkStateChgMainReload","50"]
["('EthTrcv'","EthTrcvHwAccessMonitorPeriod","1"]
["('DoIP'","DoIPControlIpAssignment","false"]
["('DoIP'","DoIPTcpTxMgtQueueSize","31"]

{"sheet":"Sheet2","index":2,"n_rows":61,"n_cols":4,"rows_kept":61,"cut":false,"hidden":false,"merged":[]}
["Module","Type","Search Pattern","Search Rule"]
["Adc","FIXED_VALUE","NA","NA"]
["Base","CUSTOM_PATTERN",".//SHORT-NAME","CONTAINS"]
["BswM","DEPENDENCY_PATTERN",".//SUB-CONTAINERS//SHORT-NAME","TEXT_EQ"]
["Can",null,null,"ATTR_EQ"]
["CanIf"]
["CanNm"]
["CanSM"]
["CanTp"]
["CanTrcv"]
["Cdd"]
["Com"]
["ComM"]
["Crc"]
["CryIf"]
["Crypto"]
["Csm"]
["Dcm"]
["Dem"]
["Det"]
["Dio"]
["DoIP"]
["E2EPW"]
["Ea"]
["EcuC"]
["EcuM"]
["Eep"]
["Eth"]
["EthIf"]
["EthSM"]
["EthSwt"]
["EthTrcv"]
["Gpt"]
["IpduM"]
["Lin"]
["LinIf"]
["LinSM"]
["LinTp"]
["LinTrcv"]
["Mcl"]
["Mcu"]
["MemIf"]
["Nm"]
["NvM"]
["Os"]
["PduR"]
["Port"]
["Resource"]
["Rte"]
["SecOC"]
["SoAd"]
["SomeIpXf"]
["Spi"]
["TcpIp"]
["vBaseEnv"]
["vBRS"]
["vLinkGen"]
["vSet"]
["Wdg"]
["WdgIf"]
["WdgM"]