{"text_format":"2","workbook":"xlsx","n_sheets":2,"sheets":["Sheet1","Sheet2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":68,"n_cols":9,"rows_kept":68,"cut":false,"hidden":false,"merged":[]}
["Hardware","Project","Module","Configuration Item","Type","Expect Value","Search Pattern","Search Text","Search Rule"]
["ALL","ALL","Dcm","DcmResetToFblAfterSessionFinalResponseEnabled","FIXED_VALUE","true","NA","NA","NA"]
["ALL","ALL","Dcm","DcmSpecificCauseCodeEnabled","FIXED_VALUE","true","NA","NA","NA"]
["ALL","ALL","Dem","DemResetConfirmedBitOnOverflow","FIXED_VALUE","false","NA","NA","NA"]
["ALL","ALL","Dem","DemPendingDtcProcessing","FIXED_VALUE","DEM_PROCESS_PDTC_ALL_DTC","NA","NA","NA"]
["ALL","ALL","Dem","DemWarningIndicatorRequestedProcessing","FIXED_VALUE","DEM_PROCESS_WIR_ALL_DTC","NA","NA","NA"]
["ALL","ALL","Dcm","DcmSpecificCauseCodeEnabled","FIXED_VALUE","true","NA","NA","NA"]
["ALL","ALL","Dem","DemClearDTCBehavior","FIXED_VALUE","DEM_CLRRESP_VOLATILE","NA","NA","NA"]
["ALL","ALL","Dem","DemMaxNumberEventEntryPrimary","FIXED_VALUE","40","NA","NA","NA"]
["ALL","ALL","Dem","DemTypeOfFreezeFrameRecordNumeration","FIXED_VALUE","DEM_FF_RECNUM_CONFIGURED","NA","NA","NA"]
["ALL","ALL","Dem","DemImmediateNvStorage","FIXED_VALUE","true","NA","NA","NA"]
["ALL","ALL","CanTp","CanTpChannelMode","FIXED_VALUE","CANTP_MODE_FULL_DUPLEX","NA","NA","NA"]
["ALL","ALL","CanTp","CanTpMainFunctionPeriod","FIXED_VALUE","0.005","NA","NA","NA"]
["ALL","ALL","CanTp","CanTpEnableSynchronousTransmit","FIXED_VALUE","true","NA","NA","NA"]
["ALL","ALL","EthIf","EthIfVlanId","FIXED_VALUE","7","NA","NA","NA"]
["ALL","ALL","EthIf","EthIfTrcvLinkStateChgMainReload","FIXED_VALUE","50","NA","NA","NA"]
["ALL","ALL","EthTrcv","EthTrcvHwAccessMonitorPeriod","FIXED_VALUE","1","NA","NA","NA"]
["ALL","ALL","DoIP","DoIPControlIpAssignment","FIXED_VALUE","false","NA","NA","NA"]
["ALL","ALL","DoIP","DoIPTcpTxMgtQueueSize","FIXED_VALUE","31","NA","NA","NA"]
["GW04","ALL","Rte","RteExclusiveAreaImplMechanism","CUSTOM_PATTERN","NONE",".//SHORT-NAME","ETHTRCV_30_88Q1010_EXCLUSIVE_AREA_SEQUENCE","CONTAINS"]
["GW04","ALL","Rte","RteExclusiveAreaImplMechanism","CUSTOM_PATTERN","NONE",".//SHORT-NAME","ETHTRCV_30_88Q1010_EXCLUSIVE_AREA_SEQUENCE","CONTAINS"]
["GW04","ALL","Rte","RteExclusiveAreaImplMechanism","CUSTOM_PATTERN","NONE",".//SHORT-NAME","EXCLUSIVE_AREA_SMI_MULTI_CHIP_ACCESS","CONTAINS"]
["GW04","ALL","TcpIp","TcpIpAssignmentTrigger","CUSTOM_PATTERN","TCPIP_MANUAL",".//SHORT-NAME","NE_CCP_MCU","CONTAINS"]
["ALL","ALL","ComM","ComMMainFunctionPeriod","FIXED_VALUE","0.01","NA","NA","NA"]
["GW04","ALL","ComM","ComMNmVariant","CUSTOM_PATTERN","FULL",".//SHORT-NAME","CNCANConnector","CONTAINS"]
["GW04","ALL","ComM","ComMNmVariant","CUSTOM_PATTERN","FULL",".//SHORT-NAME","ADCANFDConnector","CONTAINS"]
["GW04","ALL","ComM","ComMNmVariant","CUSTOM_PATTERN","FULL",".//SHORT-NAME","CHCANFDConnector","CONTAINS"]
["GW04","ALL","ComM","ComMNmVariant","CUSTOM_PATTERN","FULL",".//SHORT-NAME","CFCANConnector","CONTAINS"]
["GW04","ALL","ComM","ComMNmVariant","CUSTOM_PATTERN","LIGHT",".//SHORT-NAME","DIAGCANConnector","CONTAINS"]
["GW04","ALL","ComM","ComMNmVariant","CUSTOM_PATTERN","FULL",".//SHORT-NAME","PTEXTCAN","CONTAINS"]
["GW04","ALL","ComM","ComMNmVariant","CUSTOM_PATTERN","FULL",".//SHORT-NAME","PTCAN","CONTAINS"]
["GW04","ALL","ComM","ComMNmVariant","CUSTOM_PATTERN","LIGHT",".//SHORT-NAME","Lin2","CONTAINS"]
["GW04","ALL","ComM","ComMNmVariant","CUSTOM_PATTERN","LIGHT",".//SHORT-NAME","LIN1","CONTAINS"]
["GW04","ALL","Ea","EaNumberOfWriteCycles","FIXED_VALUE","1000000","NA","NA","NA"]
["ALL","ALL","CanIf","test_key","DEPENDENCY_PATTERN","test_value","Search Pattern","NA","Search Rule"]
["ALL","ALL","Dcm","DcmRequestManufacturerNotificationEnabled","FIXED_VALUE","true","NA","NA","NA"]
["ALL","ALL","Dcm","DcmRequestSupplierNotificationEnabled","FIXED_VALUE","true","NA","NA","NA"]
["ALL","ALL","Dcm","DcmDspSessionForBoot","CUSTOM_PATTERN","DCM_OEM_BOOT",".//SHORT-NAME","Programming","TEXT_EQ"]
["ALL","ALL","Dcm","DcmDspMaxDidToRead","FIXED_VALUE","3","NA","NA","NA"]
["ALL","ALL","Dem","DemReportSuppressedDTCsInService19x0A","FIXED_VALUE","true","NA","NA","NA"]
["ALL","ALL","Dem","DemDataElementUsePort","CUSTOM_PATTERN","USE_DATA_INTERNAL",".//SHORT-NAME","EDR_01_AgedCounter","TEXT_EQ"]
["ALL","ALL","Dem","DemDataElementUsePort","CUSTOM_PATTERN","USE_DATA_INTERNAL",".//SHORT-NAME","EDR_01_AgeingCounter","TEXT_EQ"]
["ALL","ALL","Dem","DemDataElementUsePort","CUSTOM_PATTERN","USE_DATA_INTERNAL",".//SHORT-NAME","EDR_01_FaultOccurrenceCounter","TEXT_EQ"]
["ALL","ALL","Dem","DemDataElementUsePort","CUSTOM_PATTERN","USE_DATA_INTERNAL",".//SHORT-NAME","EDR_01_FaultPendingCounter","TEXT_EQ"]
["ALL","ALL","Dem","DemDataElementInternalData","CUSTOM_PATTERN","DEM_AGED_COUNTER",".//SHORT-NAME","EDR_01_AgedCounter","TEXT_EQ"]
["ALL","ALL","Dem","DemDataElementInternalData","CUSTOM_PATTERN","DEM_AGINGCTR",".//SHORT-NAME","EDR_01_AgeingCounter","TEXT_EQ"]
["ALL","ALL","Dem","DemDataElementInternalData","CUSTOM_PATTERN","DEM_OCCCTR",".//SHORT-NAME","EDR_01_FaultOccurrenceCounter","TEXT_EQ"]
["ALL","ALL","Dem","DemDataElementInternalData","CUSTOM_PATTERN","DEM_FAULT_PENDING_COUNTER",".//SHORT-NAME","EDR_01_FaultPendingCounter","TEXT_EQ"]
["ALL","ALL","DoIP","DoIPRoutingActivationConfirmationReqLength","FIXED_VALUE","4","NA","NA","NA"]
["ALL","ALL","DoIP","DoIPRoutingActivationConfirmationResLength","FIXED_VALUE","4","NA","NA","NA"]
["ALL","ALL","DoIP","DoIPActivationLineDefaultActive","FIXED_VALUE","true","NA","NA","NA"]
["ALL","ALL","DoIP","DoIPAliveCheckResponseTimeout","FIXED_VALUE","0.5","NA","NA","NA"]
["ALL","ALL","DoIP","DoIPGeneralInactivityTime","FIXED_VALUE","300","NA","NA","NA"]
["ALL","ALL","DoIP","DoIPInitialInactivityTime","FIXED_VALUE","2","NA","NA","NA"]
["ALL","ALL","DoIP","DoIPInitialVehicleAnnouncementTime","FIXED_VALUE","0.5","NA","NA","NA"]
["ALL","ALL","DoIP","DoIPNodeType","FIXED_VALUE","DOIP_GATEWAY","NA","NA","NA"]
["ALL","ALL","DoIP","DoIPSupportEntityState","FIXED_VALUE","true","NA","NA","NA"]
["ALL","ALL","DoIP","DoIPSupportVidWithEId","FIXED_VALUE","true","NA","NA","NA"]
["ALL","ALL","DoIP","DoIPUseEIDasGID","FIXED_VALUE","true","NA","NA","NA"]
["ALL","ALL","DoIP","DoIPUseMacAddressForIdentification","FIXED_VALUE","true","NA","NA","NA"]
["ALL","ALL","DoIP","DoIPUseVehicleIdentificationSyncStatus","FIXED_VALUE","true","NA","NA","NA"]
["ALL","ALL","DoIP","DoIPVehicleAnnouncementInterval","FIXED_VALUE","0.5","NA","NA","NA"]
["ALL","ALL","DoIP","DoIPVehicleAnnouncementRepetition","FIXED_VALUE","3","NA","NA","NA"]
["GW04","ALL","Os","OsIsrInterruptSource","CUSTOM_PATTERN","211",".//SHORT-NAME","EthIsr_EthernetCnt_MCU_Ctrl_ad7672f0_EthInterruptServiceRoutine_Q0Rx","CONTAINS"]
["GW04","ALL","Os","OsIsrInterruptSource","CUSTOM_PATTERN","212",".//SHORT-NAME","EthIsr_EthernetCnt_MCU_Ctrl_ad7672f0_EthInterruptServiceRoutine_Q0Tx","CONTAINS"]
["GW04","ALL","Os","OsTaskStackSize","CUSTOM_PATTERN","2048",".//SHORT-NAME","SecureSrvTask","TEXT_EQ"]
["GW04","ALL","Os","OsTaskStackSize","CUSTOM_PATTERN","4096",".//SHORT-NAME","InitTask","TEXT_EQ"]
["GW04","ALL","Os","OsTaskStackSize","CUSTOM_PATTERN","4096",".//SHORT-NAME","User_BSW_ETH_Task_Core0","TEXT_EQ"]

{"sheet":"Sheet2","index":1,"n_rows":61,"n_cols":6,"rows_kept":61,"cut":false,"hidden":false,"merged":[]}
["Module","Type","Search Pattern","Search Rule","Hardware","Project"]
["Adc","FIXED_VALUE","NA","NA","ALL","ALL"]
["Base","CUSTOM_PATTERN",".//SHORT-NAME","CONTAINS","GW04","AS33"]
["BswM","DEPENDENCY_PATTERN",".//SUB-CONTAINERS//SHORT-NAME","TEXT_EQ","CCP","AS33P"]
["Can",null,null,"ATTR_EQ"]
["CanIf"]
["CanNm"]
["CanSM"]
["CanTp"]
["CanTrcv"]
["Cdd"]
["Com"]
["ComM"]
["Crc"]
["CryIf"]
["Crypto"]
["Csm"]
["Dcm"]
["Dem"]
["Det"]
["Dio"]
["DoIP"]
["E2EPW"]
["Ea"]
["EcuC"]
["EcuM"]
["Eep"]
["Eth"]
["EthIf"]
["EthSM"]
["EthSwt"]
["EthTrcv"]
["Gpt"]
["IpduM"]
["Lin"]
["LinIf"]
["LinSM"]
["LinTp"]
["LinTrcv"]
["Mcl"]
["Mcu"]
["MemIf"]
["Nm"]
["NvM"]
["Os"]
["PduR"]
["Port"]
["Resource"]
["Rte"]
["SecOC"]
["SoAd"]
["SomeIpXf"]
["Spi"]
["TcpIp"]
["vBaseEnv"]
["vBRS"]
["vLinkGen"]
["vSet"]
["Wdg"]
["WdgIf"]
["WdgM"]